**Quick Users Guide to the NFSEG Automated Water-Use Permit Simulation Tool:**

**Step-by-Step Procedures**

**Disclaimer**

THE SOFTWARE IS PROVIDED "AS IS", WITHOUT WARRANTY OF ANY KIND, EXPRESS OR IMPLIED, INCLUDING BUT NOT LIMITED TO THE WARRANTIES OF MERCHANTABILITY, FITNESS FOR A PARTICULAR PURPOSE AND NONINFRINGEMENT. IN NO EVENT SHALL THE AUTHORS OR COPYRIGHT HOLDERS BE LIABLE FOR ANY CLAIM, DAMAGES OR OTHER LIABILITY, WHETHER IN AN ACTION OF CONTRACT, TORT OR OTHERWISE, ARISING FROM, OUT OF OR IN CONNECTION WITH THE SOFTWARE OR THE USE OR OTHER DEALINGS IN THE SOFTWARE.

Please report any errors to Paul Bremner ([pbremner@sjrwmd.com](mailto:pbremner@sjrwmd.com)) or Lanie Meridth ([lmeridth@sjrwmd.com](mailto:lmeridth@sjrwmd.com)) at the St Johns River Water Management District, Douglas Durden ([Douglas.Durden@srwmd.org](mailto:Douglas.Durden@srwmd.org)) at the Suwannee River Water Management.

**Software Requirements:**

ArcGIS Desktop, version 10.0 or later, installed on your local machine (or a computer that you connect with remotely that has ArcGIS installed on it).

**Overview of Steps:**

Note to the User: If this is the first time running the tool or an update, please read the more detailed instructions (below) first.

1. Navigate to the top-level tool directory
2. Create a formatted User input csv file. Name is flexible, but no spaces are allowed in the name. The “user\_input\_files” folder is provided with example input files and is the recommended location for new input files.
3. Double-click on the batch file “sim\_cup\_initiate.bat” to open the tool console
4. Fill-in the User input filename, select whether to replace an existing results directory which possesses the same name as the User input file, and select a projection as prompted
5. Monitor the output in the console to ensure no errors occur, process takes about 10-20 minutes for each well depending on the size of withdrawal/injection.
6. A completion message appears at the end of a run. The console pauses to allow inspection of the output. If no errors occurred (signified by an error statement on the console) then the User has the option to either enter another User input file to run, or type **exit** to close the console. There is no limit to the number of times new input files may be processed before exiting the console. Each run is processed in its own results directory with its own logfile.
7. Each successful run generates a results directory containing an mxd map of the change in head water levels, two output csv files, and the logfile.

**NOTE:** Before clicking on the batch file to start the tool, close all related Excel and ArcMap files that are used to setup the Permitting Tool. Any open files could cause program errors. Also, it is sometimes necessary to save Excel csv files in MSDOS csv format.

**NOTE:** This tool is setup to run the NFSEG v1.1 groundwater model. Using a different model will cause unpredictable errors.

**NOTE:** The Suwanee River Water Management District (SRWMD) and St Johns River Water Management District (SJRWMD) utilize two different map projections in GIS. X,Y coordinates must correspond to the correct projection. Input the selection when prompted at the command line.

**1 = SRWMD is used for State Plane North**

**2 = SJRWMD is used for UTM Zone 17N meters**


**Detailed Instructions:**

Initial Setup / Installation of the Tool

**NOTE:** This process only needs to be done once per tool update.

**NOTE:** This tool uses the Python that is bundled with ArcMap 10.0 or newer. The tool automatically searches for the location of this Python. If that is unsuccessful, then ERRORs will occur. Ensure that ArcMap’s Python is able to be found before running the tool (see steps below).

1. Navigate to the Tool’s GitHub repository (<https://github.sjrwmd.com/pbremner/nfseg_auto_cup_tool>) and download the zip file. After the download is complete, unzip the tool to a directory on the local machine’s hard drive. The tool unzips into its own directory, referred to as the *top-level tool directory*. The portion of the default Windows PATH when unzipping is usually not necessary. Unzip the tool and enter the top-level tool directory. **NOTE:** Microsoft Edge or Firefox are the preferred browsers to use to access the District’s GitHub webpage. You may receive a security warning when visiting the page, please proceed to the webpage. If you are using Microsoft Edge, click ‘Details’ and ‘Go on to webpage’ to visit the webpage.



1. Check that the top-level tool directory includes (at a minimum) the following:

* docs *(folder)* containing this Quick Users Guide
* gis *(folder)*
* input\_and\_definition\_files *(folder)*
* model\_update.zip *(zip file)*
* src *(folder)*
* user\_input\_files *(folder)*
* sim\_cup\_initiate.bat
* setup.bat

1. Setup the tool for use by double-clicking the *setup.bat* script in the top-level directory. A message may appear warning you about running the script. Click the **Run-Anyway** option (sometimes this option only appears after clicking **More**). The setup script does the following:
   1. Search for the Python bundled with ArcGIS.
   2. Automatically generate a file called *PY\_PATH\_autogen.txt* to store the PATH. Though the simulation tool does not require the auto-generated file (the tool auto searches for Python when the file is not present), having this file available will decrease the tool runtime significantly. If Python could not be found, then a **Failure** message will appear. If this occurs, or if the version is not the one desired by the User, it will be necessary to manually set Python in the tool to resolve the issue. Please contact the tool maintainers for help.
   3. Unzip the model data directory.

How to setup the User Input File

The User input file is a comma-separated-value (.csv) file created in MS Excel, or equivalent, that lists all the wells needing to be processed for a permit. Table 1 shows an example of the Excel file format, and example csv files are also provided in the *user\_input\_files* folder included in the tool download. The name given to the file is not important, but the name must NOT contain spaces. Instead, use underscores in place of spaces. A descriptive filename of the permit simulation is recommended. The name assigned to the User input file is used to create a new results directory outside of the top-level tool directory. The results directory name appends “\_results” to the base User input file name. Within the results directory, two csv files are output summarizing the results of the simulation, both of which will be prepended with the base of the User input filename. A logfile with all output from the console is written to the results directory and named with the base User input filename. An mxd map (dh.mxd) showing the change in head in model layers 1 and 3 from the simulation is output to the results gis folder.

For example, if the input filename is:

“sim\_cup\_input\_example\_srwmd.csv”

then the results directory will be named:

“sim\_cup\_input\_example\_srwmd\_results”


and the two output csv files and log file will be named:

“sim\_cup\_input\_example\_srwmd\_delta\_q\_summary.csv”

“sim\_cup\_input\_example\_srwmd\_global\_budget\_change.csv”

“sim\_cup\_input\_example\_srwmd.log”

Example results directory:



The Rows of the User input file are as follows:

* *Row 1* contains the Permit ID and Name.
* *Row 2* contains a set of header field names describing what information needs to be filled out by the User. The field names MUST be in the order and spelling shown in the example.
* *Rows 3+* contain all the need-to-be-processed wells, one well per row.

The Columns of the well data portion (rows 3+) of the User input file are as follows:

* *Col A – WellKey –* an integer counter for each well
* *Col B – WellId –* an identifier for each well
* *Col C/D – Xcoord/Ycoord –* Cartesian coordinate representation of the Lon/Lat well coordinates. For each well, use a GIS program such as ArcMap, to obtain the X,Y coordinates within the NFSEG model.
* *Col E – layer –* model layer the well will interact with
* *Col F – Q\_mgd –* amount of water flowing through the well [units = million-gallons-per-day].


**IMPORTANT:** The Suwanee River Water Management District (SRWMD) and St Johns River Water Management District (SJRWMD) utilize two different map projections in GIS. Make note of which projection was used in GIS and input the selection when prompted at the command line.

**1 = SRWMD is used for State Plane North**

**2 = SJRWMD is used for UTM Zone 17N meters**

**NOTE:** Use a positive Q\_mgd value for withdrawal, and a negative value for injection.


Table 1 User input file example. File should be created in MS Excel, or equivalent, and be saved as a .csv file.




Running the Water-Use Simulation Permit Simulation


The Automated Water-Use Permit Simulation Tool runs a batch script within a Windows Command Prompt console. In the background, the batch script runs a Python script that controls the processing workflow and manages output. Successive input files may be processed without limit, where each new User input file is able to be entered once the current process is completed. The following are the steps to activate and run the tool:


1. Navigate to the top-level directory of the tool
2. Double click on the batch file *sim\_cup\_initiate.bat*. A console will pop-up on the screen. When first opened, the tool may take a few moments to initialize before prompting for User input.




1. Follow the prompts to input both the User input csv filename, whether to proceed with overwriting an existing results directory possessing the same name (overwrite is currently the only option), as well as the map projection that corresponds to what was used in GIS to obtain the X,Y coordinates of each well. Push Enter after each prompted input.







1. The simulation proceeds to run. Monitor the output to ensure no error messages appear. If the simulation was successful, then the output files will be written to the new results folder one level above the top-level tool directory, and a completion message will appear in the console. The output files will be prepended with the User input filename. The user will then be prompted to supply another User input file for processing. If there is no additional user input file to process, type **exit** in the command prompt or close the command terminal to exit. 

Water-Use Simulation Permit Simulation Log File

Output from the console, including any error messages, is written to a log file in the results directory that is named with the base User input filename. Error messages and warning messages usually start with one of the following terms: “ERROR”, “Warning”, or “Traceback”. If an error occurs during execution of the tool, and it is not obvious why the error occurred, then the logfile should be examined for additional information. If errors persist, the log file and a description of the issue should be emailed to the tool maintainers.

Example log file:




**Tool Operations and Results**




The NFSEG Automated Water-Use Simulation Tool uses MODFLOW to calculate changes in groundwater availability and other drawdown effects due to well additions or deletions (CUP - consumptive use permit) within the NFSEG groundwater model domain. The tool calculates the cumulative effects of adding one or more new CUP wells within the NFSEG model area, and summarizes results in the following outputs:

* Change in Water Budget
* Change in flow at river and spring flow gages
* Change in head water levels in model layers 1 and 3

The tool can be split into three stages:


1. **Preprocessing** – Processing the input CUP wells in order to setup a new MODFLOW WEL Package. The new WEL Package starts with the calibrated NFSEG 2nd Stress Period (2009), which becomes the new Stress Period 1. The new 2nd Stress Period repeats Calibrated NFSEG 2nd Stress Period plus all the CUP well modifications:



1. **Execute MODFLOW** – Utilize the new WEL Package, but all other packages are unchanged.
2. **Postprocess the results** – Extract and process the global water budget and flow changes from the *.lst* and *.hds* files.
   1. The global water budget is summarized in the *<user\_input\_filename>\_global\_budget\_change.csv* (see example):
   2. The change in flow is summarized in *<user\_input\_filename>\_delta\_q\_summary.csv* (see example): 
   3. The change in head levels of layers 1 or 3 are viewable from the *dh.mxd*: 

Lake-UFA Head Extraction

A separate, standalone tool that extracts the Lake-UFA head levels is bundled with this Tool. To navigate to the extraction tool, start from the top-level tool directory and enter into the subdirectory *src\nfseg\_lakeufahds\program:*



To use the extraction tool:

* Copy the heads file produced by the MODFLOW run into the extraction tool program directory:
  + From the results directory, copy *postproc\dh\nfseg\_auto.hds* to the tool program directory
  + Rename as *nfseg.hds*.
* Double click the Fortran executable file, *nfseg.lakeufahds.exe*, to run the extraction tool.
* Once the process is complete, the output may be moved back to the results directory.

Currently, the tool processes from three lists of lakes, and creates an output file for each of them. Each output filename has the suffix *.ufahds*. Below is an example of the input and output files.

* The input file (left) lists the NFSEG grid rows and columns, as well as the area that make up each lake. Each lake has a unique ID.
* The output file (right) lists the average UFA head levels for each Stress Period beneath each LakeID

